| # HELP: Load Existing Source Data

This panel allows the user to load multiple data types from multiple sources, i.e. the ASCII Delimited Data Files on your PC and the Kansas Geological Survey (KGS) Database & File Server. As the ASCII files are read in, the filenames are inserted into the text fields to give the user a positive feed back.
Once the user has loaded the data from the sources, select the "Add Well Data" Button to import the well / measured section data into the cross section.
NOTE: The User can load up to 3 Log ASCII Standard (LAS) version 2.0 & 3.0 files from either your PC or the KGS File Server.

## Load Geological Source Data
Select a icon button from the following list to view Help pages.
| ### Kansas Geological Survey (KGS) Database & Server Data
|  | Kansas Well Data This button allows the user to access well data stored in the Kansas database & Server. LAS ASCII Standard (LAS) version 2.0 Files Database Data: Perforations Depth Data & Formation Tops (Stratigraphic Units).
|  | Kansas Measured Sections Measured Sections (precise measurements and descriptions of a cross section of an outcrop or road cuts) for selected counties in Kansas.
| ### PC ASCII Delimited Data Files
|  | Log ASCII Standard (LAS) File Read This version will read up to 3 Log ASCII Standard (LAS) Files, versions 2.0 & 3.0. This read process does not necessarily distinguish between the two versions. The LAS Java Read classes follow the rules set up by the Canadian Well Logging Society for both versions.
|  | Tops CSV (comma delimited) ASCII File Read This version will allow the user to map a comma delimited ASCII file data columns to the tops data variables in the Profile Web Application.
|  | Geologist Report delimited ASCII File Read This version will allow the user to read & parse a delimited geologist report ASCII file data.

Author: John R. Victorine jvictor@kgs.ku.edu