12/22/98 ERRATA LIST  - "THE DESIGN, PERFORMANCE, AND ANALYSIS OF SLUG TESTS"  BY JAMES J. BUTLER, JR.

CHAPTER FIVE
	page 59, 8th line from bottom of 1st paragraph - "=0.0125" should be replaced with "= 0.0108";
	page 59, 6th line from bottom of 1st paragraph - "3.48" should be replaced with "3.69";
	page 59, 3rd line from bottom of 1st paragraph - "= 0.0125" should be replaced with "= 0.0108";
	page 59, 2nd line from bottom of 1st paragraph - "2.97" should be replaced with "4.38";
	page 63, Figure 5.4B - "= 0.0125" should be replaced with "= 0.0108";
	page 64, 2nd line from top - add "often" after "a will";
	page 69, 9th line from bottom of page - replace "3.77" with "3.88";
	page 69, 9th line from bottom of page - replace "8%"  with "5%";
	page 69, 3rd line from bottom of page - replace "30%" with "26%";
	page 75, equation (5.14a) - replace "4Krt" inside logarithmic term with "2.25Krt";
	page 79, 5th line of 3rd complete paragraph - insert "if appropriate procedures are utilized" after "pumping well";
	page 86, 6th line from bottom - "10-30" should be "10-10";
	page 93, 5th line from bottom - replace "normalized screen length the formation is.."  with "normalized screen length (b/B) is ..";
	page 94, 6th line of KGS Model section - delete "configuration";
	page 97, 5th line from top - replace "(large to moderate y)" with  "(y>0.005)";
	page 98, 8th line from top - replace "a decrease in the radial" with   "a smaller radial";

CHAPTER SIX
	page 120, 5th line from bottom - delete comma after "length".

CHAPTER SEVEN
	page 143, 11th line of first full paragraph - add "(" in front of "(1-hs)" - add ")" after "ts)";
	page 144, 9th line - change "(Cooper et al., 1967)" to "(see Chapter 5)".

CHAPTER EIGHT
	page 155, equation (8.3) should be 

	page 156, 7th line from bottom - replace "40%" with "20%";
	page 159, Table 8.3, Kr column - replace "449." with "434.";
	page 159, Table 8.3, Kr column - replace "618." with "523.";
	page 159, Table 8.3, Note at table bottom - add "Ss assumed equal to 5.5x10-5 m-1." after "in text."; 
	page 161, 8th line of 2nd complete paragraph - "" should be replaced by "";
	page 163, 11th line of 1st complete paragraph - replace "255" with "249";
	page 165, equation (8.10) - "CD(FD+1)" should be "(CD+FD)";
	page 166, FD definition - "" should be replaced by "";
	page 167, Figure 8.10 Figure Caption - "Logarithm of normalized head .." should be replaced by "Normalized head ...".

CHAPTER NINE
	page 179, line 9 of paragraph beginning "Karasaki (1990).." - replace "Thus, similar to" with "Note that for both the drillstem test and";
	page 180, line 16 - "underestimation" should be "overestimation";
	page 180, line 1 of 3rd complete paragraph - replace "significance of the estimate" with "significance of the magnitude";
	page 180, line 3 of 3rd complete paragraph - add "often" before "an indication".

CHAPTER TEN
	page 191, line 6 - replace "1.06 m/d and 8.5" with "1.16 m/d and 9.35";
	page 200, 1st line below equation (10.7c) - replace "wellbore storage" with "a";
	page 201, line 12 - "48%" should be "35%";
	page 201, line 14 - "22%" should be "30%".

CHAPTER ELEVEN
	p. 209, Figure 11.2 - quantity plotted on x axis is actually 4lflf.

CHAPTER TWELVE
	page 220, 5th line of 3rd complete paragraph - replace "very reasonable" with "relatively good";
	page 222, 3rd line of 2nd complete paragraph - replace "very reasonable" with "relatively good";
	page 225, Figure 12.5 - printing error - "Kr" not clear on left bottom and upper right;
	page 226, Figure 12.6 - replace "rw" with "a"
					  - replace "row" with "aow";
	page 227, 12th line from bottom - replace "effective screen radii" with "dimensionless storage parameter (a)";
	page 227, 10th line from bottom - replace "effective screen radii" with "a".